(module PhoenixContact_MSTB_2,5_2-GF_1x02_P5.00mm_Horizontal_ThreadedFlange_MountHole (layer F.Cu) (tedit 5B785046)
  (descr "Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF; number of pins: 02; pin pitch: 5.00mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776692 12A || order number: 1923979 16A (HC)")
  (tags "phoenix_contact connector MSTB_01x02_GF_5.00mm_MH")
  (fp_text reference REF** (at 2.5 -3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PhoenixContact_MSTB_2,5_2-GF_1x02_P5.00mm_Horizontal_ThreadedFlange_MountHole (at 2.5 11.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -5 2.5) (end -2.79 2.5) (layer B.SilkS) (width 0.12))
  (fp_circle (center 10 2.5) (end 12.21 2.5) (layer B.SilkS) (width 0.12))
  (fp_circle (center 10 2.5) (end 12.1 2.5) (layer B.Fab) (width 0.1))
  (fp_circle (center -5 2.5) (end -2.9 2.5) (layer B.Fab) (width 0.1))
  (fp_circle (center 10 2.5) (end 12.6 2.5) (layer B.CrtYd) (width 0.05))
  (fp_circle (center -5 2.5) (end -2.4 2.5) (layer B.CrtYd) (width 0.05))
  (fp_line (start -7.61 -2.11) (end -7.61 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.61 10.11) (end 12.61 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.61 10.11) (end 12.61 -2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.61 -2.11) (end -7.61 -2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.5 -2) (end -7.5 10) (layer F.Fab) (width 0.1))
  (fp_line (start -7.5 10) (end 12.5 10) (layer F.Fab) (width 0.1))
  (fp_line (start 12.5 10) (end 12.5 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 12.5 -2) (end -7.5 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -7.61 8.61) (end -7.61 6.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.61 6.81) (end 12.61 6.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.61 6.81) (end 12.61 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.61 8.61) (end -7.61 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 10.11) (end -4 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 10.11) (end -4.25 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.25 8.61) (end -5.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.75 8.61) (end -6 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 9 10.11) (end 11 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 10.11) (end 10.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.75 8.61) (end 9.25 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.25 8.61) (end 9 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 10.11) (end 1 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 10.11) (end 0.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.75 8.61) (end -0.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 8.61) (end -1 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 10.11) (end 6 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 10.11) (end 5.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.75 8.61) (end 4.25 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.25 8.61) (end 4 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -8 -2.5) (end -8 10.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8 10.5) (end 13 10.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13 10.5) (end 13 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13 -2.5) (end -8 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.3 -2.91) (end 0 -2.31) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -2.31) (end -0.3 -2.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 -2.91) (end 0.3 -2.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.95 -2) (end 0 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -0.5) (end -0.95 -2) (layer F.Fab) (width 0.1))
  (pad 1 thru_hole roundrect (at 0 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.125))
  (pad 2 thru_hole oval (at 5 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 10 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.5 -1.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTB_2,5_2-GF_1x02_P5.00mm_Horizontal_ThreadedFlange_MountHole.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)