(module PhoenixContact_MSTBA_2,5_2-G_1x02_P5.00mm_Horizontal (layer F.Cu) (tedit 5B785046)
  (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G; number of pins: 02; pin pitch: 5.00mm; Angled || order number: 1757475 12A || order number: 1923759 16A (HC)")
  (tags "phoenix_contact connector MSTBA_01x02_G_5.00mm")
  (fp_text reference REF** (at 2.5 -3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PhoenixContact_MSTBA_2,5_2-G_1x02_P5.00mm_Horizontal (at 2.5 11.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.61 -2.11) (end -3.61 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.61 10.11) (end 8.61 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.61 10.11) (end 8.61 -2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.61 -2.11) (end -3.61 -2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.5 -2) (end -3.5 10) (layer F.Fab) (width 0.1))
  (fp_line (start -3.5 10) (end 8.5 10) (layer F.Fab) (width 0.1))
  (fp_line (start 8.5 10) (end 8.5 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 8.5 -2) (end -3.5 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -3.61 8.61) (end -3.61 6.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.61 6.81) (end 8.61 6.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.61 6.81) (end 8.61 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.61 8.61) (end -3.61 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 10.11) (end 1 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 10.11) (end 0.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.75 8.61) (end -0.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 8.61) (end -1 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 10.11) (end 6 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 10.11) (end 5.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.75 8.61) (end 4.25 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.25 8.61) (end 4 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 -2.5) (end -4 10.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4 10.5) (end 9 10.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9 10.5) (end 9 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9 -2.5) (end -4 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.3 -2.91) (end 0 -2.31) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -2.31) (end -0.3 -2.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 -2.91) (end 0.3 -2.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.95 -2) (end 0 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -0.5) (end -0.95 -2) (layer F.Fab) (width 0.1))
  (pad 1 thru_hole roundrect (at 0 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.125))
  (pad 2 thru_hole oval (at 5 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.5 -1.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G_1x02_P5.00mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)