(module PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole (layer F.Cu) (tedit 5B785047)
  (descr "Generic Phoenix Contact connector footprint for: MSTB_2,5/2-GF-5,08; number of pins: 02; pin pitch: 5.08mm; Angled; threaded flange; footprint includes mount hole for mounting screw: ISO 1481-ST 2.2x6.5 C or ISO 7049-ST 2.2x6.5 C (http://www.fasteners.eu/standards/ISO/7049/) || order number: 1776508 12A || order number: 1924088 16A (HC)")
  (tags "phoenix_contact connector MSTB_01x02_GF_5.08mm_MH")
  (fp_text reference REF** (at 2.54 -3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole (at 2.54 11.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -5.08 2.5) (end -2.87 2.5) (layer B.SilkS) (width 0.12))
  (fp_circle (center 10.16 2.5) (end 12.37 2.5) (layer B.SilkS) (width 0.12))
  (fp_circle (center 10.16 2.5) (end 12.26 2.5) (layer B.Fab) (width 0.1))
  (fp_circle (center -5.08 2.5) (end -2.98 2.5) (layer B.Fab) (width 0.1))
  (fp_circle (center 10.16 2.5) (end 12.76 2.5) (layer B.CrtYd) (width 0.05))
  (fp_circle (center -5.08 2.5) (end -2.48 2.5) (layer B.CrtYd) (width 0.05))
  (fp_line (start -7.73 -2.11) (end -7.73 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.73 10.11) (end 12.81 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.81 10.11) (end 12.81 -2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.81 -2.11) (end -7.73 -2.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.62 -2) (end -7.62 10) (layer F.Fab) (width 0.1))
  (fp_line (start -7.62 10) (end 12.7 10) (layer F.Fab) (width 0.1))
  (fp_line (start 12.7 10) (end 12.7 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 12.7 -2) (end -7.62 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -7.73 8.61) (end -7.73 6.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.73 6.81) (end 12.81 6.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.81 6.81) (end 12.81 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.81 8.61) (end -7.73 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.08 10.11) (end -4.08 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.08 10.11) (end -4.33 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.33 8.61) (end -5.83 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.83 8.61) (end -6.08 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.16 10.11) (end 11.16 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.16 10.11) (end 10.91 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.91 8.61) (end 9.41 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.41 8.61) (end 9.16 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 10.11) (end 1 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 10.11) (end 0.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.75 8.61) (end -0.75 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.75 8.61) (end -1 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.08 10.11) (end 6.08 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.08 10.11) (end 5.83 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.83 8.61) (end 4.33 8.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.33 8.61) (end 4.08 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.12 -2.5) (end -8.12 10.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.12 10.5) (end 13.2 10.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.2 10.5) (end 13.2 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.2 -2.5) (end -8.12 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.3 -2.91) (end 0 -2.31) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -2.31) (end -0.3 -2.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 -2.91) (end 0.3 -2.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.95 -2) (end 0 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -0.5) (end -0.95 -2) (layer F.Fab) (width 0.1))
  (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192))
  (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5.08 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 10.16 2.5) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.54 -1.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTB_2,5_2-GF-5,08_1x02_P5.08mm_Horizontal_ThreadedFlange_MountHole.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)