(module PhoenixContact_MSTBV_2,5_6-GF_1x06_P5.00mm_Vertical_ThreadedFlange (layer F.Cu) (tedit 5B785046)
  (descr "Generic Phoenix Contact connector footprint for: MSTBV_2,5/6-GF; number of pins: 06; pin pitch: 5.00mm; Vertical; threaded flange || order number: 1776922 12A || order number: 1924457 16A (HC)")
  (tags "phoenix_contact connector MSTBV_01x06_GF_5.00mm")
  (fp_text reference REF** (at 12.5 -6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PhoenixContact_MSTBV_2,5_6-GF_1x06_P5.00mm_Vertical_ThreadedFlange (at 12.5 5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 0 0.55) (end -2 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
  (fp_arc (start 5 0.55) (end 3 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
  (fp_arc (start 10 0.55) (end 8 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
  (fp_arc (start 15 0.55) (end 13 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
  (fp_arc (start 20 0.55) (end 18 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
  (fp_arc (start 25 0.55) (end 23 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
  (fp_circle (center -5 0) (end -3.1 0) (layer F.SilkS) (width 0.12))
  (fp_circle (center 30 0) (end 31.9 0) (layer F.SilkS) (width 0.12))
  (fp_circle (center -5 0) (end -4 0) (layer F.SilkS) (width 0.12))
  (fp_circle (center 30 0) (end 31 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.61 -4.91) (end -7.61 3.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.61 3.91) (end 32.61 3.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 32.61 3.91) (end 32.61 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 32.61 -4.91) (end -7.61 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.5 -4.8) (end -7.5 3.8) (layer F.Fab) (width 0.1))
  (fp_line (start -7.5 3.8) (end 32.5 3.8) (layer F.Fab) (width 0.1))
  (fp_line (start 32.5 3.8) (end 32.5 -4.8) (layer F.Fab) (width 0.1))
  (fp_line (start 32.5 -4.8) (end -7.5 -4.8) (layer F.Fab) (width 0.1))
  (fp_line (start -7.61 -4.1) (end -6.11 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 32.61 -4.1) (end 31.11 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 -4.1) (end 4 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 -4.1) (end 9 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -4.1) (end 14 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 16 -4.1) (end 19 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 21 -4.1) (end 24 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 -3.1) (end -6 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 -4.91) (end -4 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 -4.91) (end -4 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 -3.1) (end -6 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 29 -3.1) (end 29 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 29 -4.91) (end 31 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 31 -4.91) (end 31 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 31 -3.1) (end 29 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 -4.1) (end -1 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 26 -4.1) (end 29 -4.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 -3.1) (end -1 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 -4.91) (end 1 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 -4.91) (end 1 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 -3.1) (end -1 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 -3.1) (end 4 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 -4.91) (end 6 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 -4.91) (end 6 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 -3.1) (end 4 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 9 -3.1) (end 9 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 9 -4.91) (end 11 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -4.91) (end 11 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 11 -3.1) (end 9 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 14 -3.1) (end 14 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 14 -4.91) (end 16 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 16 -4.91) (end 16 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 16 -3.1) (end 14 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 19 -3.1) (end 19 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 19 -4.91) (end 21 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 21 -4.91) (end 21 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 21 -3.1) (end 19 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 24 -3.1) (end 24 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 24 -4.91) (end 26 -4.91) (layer F.SilkS) (width 0.12))
  (fp_line (start 26 -4.91) (end 26 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 26 -3.1) (end 24 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2 2.2) (end 3 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 7 2.2) (end 8 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 12 2.2) (end 13 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 17 2.2) (end 18 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 22 2.2) (end 23 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 2.2) (end -2.7 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.7 2.2) (end -2.7 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.7 -3.1) (end 27.7 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 27.7 -3.1) (end 27.7 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 27.7 2.2) (end 27 2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -8 -5.3) (end -8 4.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8 4.3) (end 33 4.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 33 4.3) (end 33 -5.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 33 -5.3) (end -8 -5.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.3 -5.71) (end 0 -5.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -5.11) (end -0.3 -5.71) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.3 -5.71) (end 0.3 -5.71) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.5 -3.55) (end 0 -2.55) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -2.55) (end -0.5 -3.55) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -3.55) (end 0.5 -3.55) (layer F.Fab) (width 0.1))
  (pad 1 thru_hole roundrect (at 0 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.125))
  (pad 2 thru_hole oval (at 5 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 10 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 15 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 20 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 25 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask))
  (fp_text user %R (at 12.5 -4.1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBV_2,5_6-GF_1x06_P5.00mm_Vertical_ThreadedFlange.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)