(module raspberrypi_2_3 (layer F.Cu) (tedit 5C5E4138)
  (descr "RaspberryPi 2")
  (tags CONN)
  (fp_text reference RP? (at 0 -8.9) (layer F.Fab)
    (effects (font (size 2 2) (thickness 0.25)))
  )
  (fp_text value Raspberry_Pi_2_3 (at 0.1 -5.7) (layer F.Fab)
    (effects (font (size 2 2) (thickness 0.25)))
  )
  (fp_text user "By Lukaneco" (at 23.7 -6.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 25.39492 2.54) (end 25.39492 -2.54) (layer F.Fab) (width 0.15))
  (fp_line (start -25.4 -2.54) (end -25.4 2.54) (layer F.Fab) (width 0.15))
  (fp_line (start 25.4 2.54) (end -25.4 2.54) (layer F.Fab) (width 0.15))
  (fp_line (start -25.4 -2.54) (end 25.4 -2.54) (layer F.Fab) (width 0.15))
  (fp_arc (start -29 0) (end -32.5 0) (angle 90) (layer F.Fab) (width 0.15))
  (fp_arc (start -29 49) (end -29 52.5) (angle 90) (layer F.Fab) (width 0.15))
  (fp_line (start -29 52.5) (end 49.5 52.5) (layer F.Fab) (width 0.15))
  (fp_arc (start 49.5 49.5) (end 52.5 49.5) (angle 90) (layer F.Fab) (width 0.15))
  (fp_line (start 52.5 49.5) (end 52.5 -0.5) (layer F.Fab) (width 0.15))
  (fp_arc (start 49.5 -0.5) (end 49.5 -3.5) (angle 90) (layer F.Fab) (width 0.15))
  (fp_line (start 49.5 -3.5) (end -29 -3.5) (layer F.Fab) (width 0.15))
  (fp_line (start -32.5 49) (end -32.5 0) (layer F.Fab) (width 0.15))
  (fp_line (start 37.5 -1) (end 54.6 -1) (layer B.CrtYd) (width 0.15))
  (fp_line (start 54.6 12.1) (end 54.6 -1) (layer B.CrtYd) (width 0.15))
  (fp_line (start 37.5 -1) (end 37.5 12.1) (layer B.CrtYd) (width 0.15))
  (fp_line (start 54.6 12.1) (end 37.5 12.1) (layer B.CrtYd) (width 0.15))
  (fp_line (start 54.6 30.1) (end 54.6 17) (layer B.CrtYd) (width 0.15))
  (fp_line (start 54.6 30.1) (end 37.5 30.1) (layer B.CrtYd) (width 0.15))
  (fp_line (start 37.5 30.1) (end 37.5 17) (layer B.CrtYd) (width 0.15))
  (fp_line (start 37.5 17) (end 54.6 17) (layer B.CrtYd) (width 0.15))
  (fp_line (start 33.6 34.3) (end 54.6 34.3) (layer B.CrtYd) (width 0.15))
  (fp_line (start 54.6 50.2) (end 33.6 50.2) (layer B.CrtYd) (width 0.15))
  (fp_line (start 33.6 50.2) (end 33.6 34.3) (layer B.CrtYd) (width 0.15))
  (fp_line (start 54.6 50.2) (end 54.6 34.3) (layer B.CrtYd) (width 0.15))
  (fp_line (start -17.9 16.4) (end -17.9 31) (layer B.CrtYd) (width 0.15))
  (fp_line (start -17.9 31) (end -32.5 31) (layer B.CrtYd) (width 0.15))
  (fp_line (start -17.9 16.4) (end -32.5 16.4) (layer B.CrtYd) (width 0.15))
  (fp_line (start 24 55) (end 24 37) (layer B.CrtYd) (width 0.15))
  (fp_line (start 24 37) (end 18 37) (layer B.CrtYd) (width 0.15))
  (fp_line (start 18 37) (end 18 55) (layer B.CrtYd) (width 0.15))
  (fp_line (start 18 55) (end 24 55) (layer B.CrtYd) (width 0.15))
  (fp_line (start 7 52.5) (end 7 41.8) (layer B.CrtYd) (width 0.15))
  (fp_line (start -8 41.8) (end 7 41.8) (layer B.CrtYd) (width 0.15))
  (fp_line (start -8 41.8) (end -8 52.5) (layer B.CrtYd) (width 0.15))
  (fp_line (start -25.7 52.5) (end -25.7 47.5) (layer B.CrtYd) (width 0.15))
  (fp_line (start -18.2 52.5) (end -18.2 47.5) (layer B.CrtYd) (width 0.15))
  (fp_line (start -18.2 47.5) (end -25.7 47.5) (layer B.CrtYd) (width 0.15))
  (fp_line (start 7 52.5) (end -8 52.5) (layer B.CrtYd) (width 0.15))
  (fp_line (start -18.2 52.5) (end -25.7 52.5) (layer B.CrtYd) (width 0.15))
  (fp_line (start -32.5 16.4) (end -32.5 31) (layer B.CrtYd) (width 0.15))
  (pad "" np_thru_hole circle (at 29 49) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -29 49) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 29 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -29 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask F.SilkS))
  (pad 39 thru_hole circle (at 24.13 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 40 thru_hole circle (at 24.13 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 37 thru_hole circle (at 21.59 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 38 thru_hole circle (at 21.59 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 35 thru_hole circle (at 19.05 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 36 thru_hole circle (at 19.05 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 33 thru_hole circle (at 16.51 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 34 thru_hole circle (at 16.51 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 31 thru_hole circle (at 13.97 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 32 thru_hole circle (at 13.97 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 26 thru_hole circle (at 6.35 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 25 thru_hole circle (at 6.35 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 22 thru_hole circle (at 1.27 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 21 thru_hole circle (at 1.27 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 20 thru_hole circle (at -1.27 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 19 thru_hole circle (at -1.27 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 18 thru_hole circle (at -3.81 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 17 thru_hole circle (at -3.81 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 16 thru_hole circle (at -6.35 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 15 thru_hole circle (at -6.35 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 14 thru_hole circle (at -8.89 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 13 thru_hole circle (at -8.89 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 12 thru_hole circle (at -11.43 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole circle (at -11.43 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole circle (at -13.97 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole circle (at -13.97 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole circle (at -16.51 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at -16.51 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at -19.05 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -19.05 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at -21.59 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at -21.59 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -24.13 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole rect (at -24.13 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 23 thru_hole circle (at 3.81 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 24 thru_hole circle (at 3.81 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 30 thru_hole circle (at 11.43 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 29 thru_hole circle (at 11.43 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 28 thru_hole circle (at 8.89 -1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 27 thru_hole circle (at 8.89 1.27) (size 1.75 1.75) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (model unsorted/raspberryPi3b-simple.wrl
    (offset (xyz 9.905999851226808 -24.5871996307373 -18.28799972534179))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 180))
  )
  (model Pin_Header/Pin_Header_Straight_Female_2x20_RaspPi.wrl
    (offset (xyz 0 0 -6.349999904632568))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 90))
  )
)
