{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["bq24600","bq24610_bq24617","BQ24616","bq24618","bq24620","bq24630","bq24640","bq24650","103AT"],"not_rendered":{"images":94,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"bq24600","index":0,"n_rows":70,"n_cols":11,"rows_kept":70,"merged":[[16,1,16,3],[25,1,25,3],[31,1,31,3],[32,1,32,3],[40,1,40,3],[49,1,49,3],[52,5,52,7],[54,1,54,3],[58,1,58,3],[68,1,68,3]],"flags":["formulas_cached_only"]}
[null,"Li-ion charger bq24600 typical application circuit"]
{"$rows_empty":20}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Battery charge voltage setting"]
[null,"Cell count",5,"cell"]
[null,"Vcell",4.2,"V/cell"]
[null,"Vbat",21,"V"]
[null,"R1",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R2",900,"k-ohm"]
[]
[null,"Battery fast-charge current setting"]
[null,"Ichg",3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET",0.6,"V",null,"Iprechg=Iterm=Ichg/10"]
[null,"R7",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R8",{"v":22.22222222222222,"d":"22.22"},"k-ohm"]
[]
[null,"Iripple_Lout",{"$nulls":3},"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Vin",28,"V",null,"Charge Current","2A","4A","6A","8A","10A"]
[null,"Vout  (Vbat)",21,"V",null,"Output Inductor Lo","3.3mH","3.3mH","2.2mH","2.2mH","1.5mH"]
[null,"Duty",{"v":0.75,"d":"0.750"},null,null,"Output Capacitor Co","20mF","20mF","30mF","40mF","40mF"]
[null,"Fs",1200,"kHz",null,"Sense Resistor","10mW","10mW","10mW","10mW","10mW"]
[null,"Lout",{"v":3.3,"d":"3.30"},"uH"]
[null,"IRIPPLE",{"v":1.325757575757576,"d":"1.33"},"A"]
[null,"VRIPPLE",{"v":6.904987373737374,"d":"6.90"},"mV"]
[]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":3.3,"d":"3.30"},"uH"]
[null,"Cout",{"v":20,"d":"20.00"},"uF"]
[null,"f0",{"v":19.590573430629732,"d":"19.59"},"kHz",null,"recommended range 16~28 kHz"]
[]
[null,"Timer (fixed)"]
[null,"Tprecharge",{"v":30,"d":"30.00"},"min"]
[null,"Tfastcharge",5,"hr"]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","0-45C"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (45C)",{"v":4.911,"d":"4.91"},"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VLTF",{"v":2.4255,"d":"2.43"},{"v":0.735,"d":"73.50%"}]
[null,"VTCO",{"v":1.1351999999999998,"d":"1.14"},{"v":0.344,"d":"34.40%"}]
[null,"R9",{"v":9.261870542032382,"d":"9.26"},"9.31 k-ohm"]
[null,"R10",{"v":440.35294825762367,"d":"440.35"},"430 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24600",32,"V"]

{"sheet":"bq24610_bq24617","index":1,"n_rows":96,"n_cols":11,"rows_kept":96,"merged":[[17,1,17,3],[30,1,30,3],[37,1,37,3],[45,1,45,3],[52,1,52,3],[53,1,53,3],[61,1,61,3],[70,1,70,3],[73,5,73,7],[75,1,75,3],[78,1,78,3],[83,1,83,3],[93,1,93,3]],"flags":["formulas_cached_only"]}
[null,"Li-ion charger bq24610 typical application circuit"]
{"$rows_empty":25}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Battery charge voltage setting"]
[null,"Cell count",3,"cell"]
[null,"Vcell",4.2,"V/cell"]
[null,"Vbat",12.600000000000001,"V"]
[null,"R1",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R2",500,"k-ohm"]
[]
[null,"Adaptor regulation current"]
[null,"Iadp",4,"A"]
[null,"RAC",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ACSET",{"v":0.8,"d":"0.800"},"V"]
[null,"R3",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R4",{"v":32.00000000000001,"d":"32.00"},"k-ohm"]
[]
[null,"Battery pre-charge/termination current setting"]
[null,"Iprechg (Iterm)",0.3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET2",0.3,"V"]
[null,"R5",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R6",{"v":10,"d":"10.00"},"k-ohm"]
[]
[null,"Battery fast-charge current setting"]
[null,"Ichg",3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET1",0.6,"V"]
[null,"R7",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R8",{"v":22.22222222222222,"d":"22.22"},"k-ohm"]
[]
[null,"Iripple_Lout_Vripple",{"$nulls":3},"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Vin",19,"V",null,"Charge Current","2A","4A","6A","8A","10A"]
[null,"Vout  (Vbat)",12.600000000000001,"V",null,"Output Inductor Lo","6.8mH","6.8mH","4.7mH","3.3mH","3.3mH"]
[null,"Duty",{"v":0.6631578947368422,"d":"0.663"},null,null,"Output Capacitor Co","20mF","20mF","30mF","40mF","40mF"]
[null,"Fs",600,"(kHz)",null,"Sense Resistor","10mW","10mW","10mW","10mW","10mW"]
[null,"Lout",{"v":6.8,"d":"6.80"},"(uH)"]
[null,"IRIPPLE",{"v":1.0402476780185756,"d":"1.04"},"A"]
[null,"VRIPPLE",{"v":10.835913312693496,"d":"10.84"},"mV"]
[]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":6.8,"d":"6.80"},"(uH)"]
[null,"Cout",{"v":20,"d":"20.00"},"(uF)"]
[null,"f0",{"v":13.647391865809526,"d":"13.65"},"kHz",null,"recommended range 12~17 kHz"]
[]
[null,"Precharge timer (fixed)"]
[null,"Tprecharge",{"v":30,"d":"30.00"},"min"]
[]
[null,"Fastcharge timer"]
[null,"Kttc",{"v":5.6,"d":"5.60"},"min/nF"]
[null,"Cttc",56,"nF"]
[null,"Tcharge",{"v":5.226666666666666,"d":"5.23"},"hr"]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","(0-45C)"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (45C)",{"v":4.911,"d":"4.91"},"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VLTF",{"v":2.4255,"d":"2.43"},{"v":0.735,"d":"73.50%"}]
[null,"VTCO",{"v":1.1351999999999998,"d":"1.14"},{"v":0.344,"d":"34.40%"}]
[null,"R9",{"v":9.261870542032382,"d":"9.26"},"9.31 k-ohm"]
[null,"R10",{"v":440.35294825762367,"d":"440.35"},"430 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24610",32,"V"]
[null,"bq24617",26,"V"]

{"sheet":"BQ24616","index":2,"n_rows":95,"n_cols":11,"rows_kept":95,"merged":[[17,1,17,3],[30,1,30,3],[37,1,37,3],[45,1,45,3],[52,1,52,3],[53,1,53,3],[61,1,61,3],[70,1,70,3],[73,5,73,7],[75,1,75,3],[78,1,78,3],[83,1,83,3],[93,1,93,3]],"flags":["formulas_cached_only"]}
[null,"Li-ion charger bq24616 typical application circuit (JEITA compatible)"]
{"$rows_empty":25}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Battery charge voltage setting"]
[null,"Cell count",3,"cell"]
[null,"Vcell",4.2,"V/cell"]
[null,"Vbat",12.600000000000001,"V"]
[null,"R1",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R2",500,"k-ohm"]
[]
[null,"Adaptor regulation current"]
[null,"Iadp",4,"A"]
[null,"RAC",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ACSET",{"v":0.8,"d":"0.800"},"V"]
[null,"R3",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R4",{"v":32.00000000000001,"d":"32.00"},"k-ohm"]
[]
[null,"Battery pre-charge/termination current setting"]
[null,"Iprechg (Iterm)",0.3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET2",0.3,"V"]
[null,"R5",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R6",{"v":10,"d":"10.00"},"k-ohm"]
[]
[null,"Battery fast-charge current setting"]
[null,"Ichg",3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET1",0.6,"V"]
[null,"R7",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R8",{"v":22.22222222222222,"d":"22.22"},"k-ohm"]
[]
[null,"Iripple_Lout_Vripple",{"$nulls":3},"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Vin",19,"V",null,"Charge Current","2A","4A","6A","8A","10A"]
[null,"Vout  (Vbat)",12.600000000000001,"V",null,"Output Inductor Lo","6.8mH","6.8mH","4.7mH","3.3mH","3.3mH"]
[null,"Duty",{"v":0.6631578947368422,"d":"0.663"},null,null,"Output Capacitor Co","20mF","20mF","30mF","40mF","40mF"]
[null,"Fs",600,"(kHz)",null,"Sense Resistor","10mW","10mW","10mW","10mW","10mW"]
[null,"Lout",{"v":6.8,"d":"6.80"},"(uH)"]
[null,"IRIPPLE",{"v":1.0402476780185756,"d":"1.04"},"A"]
[null,"VRIPPLE",{"v":20.944437398905254,"d":"20.94"},"mV"]
[]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":6.8,"d":"6.80"},"(uH)"]
[null,"Cout",{"v":20,"d":"20.00"},"(uF)"]
[null,"f0",{"v":13.647391865809526,"d":"13.65"},"kHz",null,"recommended range 12~17 kHz"]
[]
[null,"Precharge timer (fixed)"]
[null,"Tprecharge",{"v":30,"d":"30.00"},"min"]
[]
[null,"Fastcharge timer"]
[null,"Kttc",{"v":5.6,"d":"5.60"},"min/nF"]
[null,"Cttc",56,"nF"]
[null,"Tcharge",{"v":5.226666666666666,"d":"5.23"},"hr"]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","0-60C"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (60C)",3.02,"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VCOOL",{"v":2.3331,"d":"2.33"},{"v":0.707,"d":"70.70%"}]
[null,"VWARM",{"v":1.5839999999999999,"d":"1.58"},{"v":0.48,"d":"48.00%"}]
[null,"R9",{"v":2.271567876373081,"d":"2.27"},"2.2 k-ohm"]
[null,"R10",{"v":6.85945733884236,"d":"6.86"},"6.8 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24616",32,"V"]

{"sheet":"bq24618","index":3,"n_rows":95,"n_cols":11,"rows_kept":95,"merged":[[17,1,17,3],[30,1,30,3],[37,1,37,3],[45,1,45,3],[52,1,52,3],[53,1,53,3],[61,1,61,3],[70,1,70,3],[73,5,73,7],[75,1,75,3],[78,1,78,3],[83,1,83,3],[93,1,93,3]],"flags":["formulas_cached_only"]}
[null,"Li-ion charger bq24618 typical application circuit"]
{"$rows_empty":25}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Battery charge voltage setting"]
[null,"Cell count",1,"cell"]
[null,"Vcell",4.2,"V/cell"]
[null,"Vbat",4.2,"V"]
[null,"R1",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R2",100,"k-ohm"]
[]
[null,"Adaptor regulation current"]
[null,"Iadp",2,"A"]
[null,"RAC",20,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ACSET",{"v":0.8,"d":"0.800"},"V"]
[null,"R3",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R4",{"v":32.00000000000001,"d":"32.00"},"k-ohm"]
[]
[null,"Battery pre-charge/termination current setting"]
[null,"Iprechg (Iterm)",0.3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET2",0.3,"V"]
[null,"R5",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R6",{"v":10,"d":"10.00"},"k-ohm"]
[]
[null,"Battery fast-charge current setting"]
[null,"Ichg",2,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET1",0.4,"V"]
[null,"R7",{"v":232,"d":"232.0"},"k-ohm"]
[null,"R8",{"v":32.00000000000001,"d":"32.00"},"k-ohm"]
[]
[null,"Iripple_Lout_Vripple",{"$nulls":3},"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Vin",5,"V",null,"Charge Current","2A","4A","6A","8A","10A"]
[null,"Vout  (Vbat)",4.2,"V",null,"Output Inductor Lo","6.8mH","6.8mH","4.7mH","3.3mH","3.3mH"]
[null,"Duty",{"v":0.8400000000000001,"d":"0.840"},null,null,"Output Capacitor Co","20mF","20mF","30mF","40mF","40mF"]
[null,"Fs",600,"(kHz)",null,"Sense Resistor","10mW","10mW","10mW","10mW","10mW"]
[null,"Lout",{"v":6.8,"d":"6.80"},"(uH)"]
[null,"IRIPPLE",{"v":0.16470588235294115,"d":"0.16"},"A"]
[null,"VRIPPLE",{"v":1.7156862745098043,"d":"1.72"},"mV"]
[]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":6.8,"d":"6.80"},"(uH)"]
[null,"Cout",{"v":20,"d":"20.00"},"(uF)"]
[null,"f0",{"v":13.647391865809526,"d":"13.65"},"kHz",null,"recommended range 12~17 kHz"]
[]
[null,"Precharge timer (fixed)"]
[null,"Tprecharge",{"v":30,"d":"30.00"},"min"]
[]
[null,"Fastcharge timer"]
[null,"Kttc",{"v":5.6,"d":"5.60"},"min/nF"]
[null,"Cttc",33,"nF"]
[null,"Tcharge",{"v":3.0799999999999996,"d":"3.08"},"hr"]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","(0-45C)"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (45C)",{"v":4.911,"d":"4.91"},"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VLTF",{"v":2.4255,"d":"2.43"},{"v":0.735,"d":"73.50%"}]
[null,"VTCO",{"v":1.1351999999999998,"d":"1.14"},{"v":0.344,"d":"34.40%"}]
[null,"R9",{"v":9.261870542032382,"d":"9.26"},"9.31 k-ohm"]
[null,"R10",{"v":440.35294825762367,"d":"440.35"},"430 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24618",32,"V"]

{"sheet":"bq24620","index":4,"n_rows":70,"n_cols":11,"rows_kept":70,"merged":[[16,1,16,3],[25,1,25,3],[31,1,31,3],[32,1,32,3],[40,1,40,3],[49,1,49,3],[52,5,52,7],[54,1,54,3],[58,1,58,3],[68,1,68,3]],"flags":["formulas_cached_only"]}
[null,"LiFePO4 charger bq24620 typical application circuit"]
{"$rows_empty":20}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Battery charge voltage setting"]
[null,"Cell count",5,"cell"]
[null,"Vcell",3.6,"V/cell"]
[null,"Vbat",18,"V"]
[null,"R1",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R2",900,"k-ohm"]
[]
[null,"Battery fast-charge current setting"]
[null,"Ichg",3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET",0.6,"V",null,"Iterm=Ichg/10"]
[null,"R7",{"v":100,"d":"100.0"},"k-ohm",null,"Fixed Iprechg=125mA for 10mΩ sensing resistor"]
[null,"R8",{"v":22.22222222222222,"d":"22.22"},"k-ohm"]
[]
[null,"Iripple_Lout",{"$nulls":3},"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Vin",28,"V",null,"Charge Current","2A","4A","6A","8A","10A"]
[null,"Vout  (Vbat)",18,"V",null,"Output Inductor Lo","8.2mH","8.2mH","5.6mH","4.7mH","4.7mH"]
[null,"Duty",{"v":0.6428571428571429,"d":"0.643"},null,null,"Output Capacitor Co","20mF","20mF","30mF","40mF","40mF"]
[null,"Fs",300,"kHz",null,"Sense Resistor","10mW","10mW","10mW","10mW","10mW"]
[null,"Lout",{"v":8.2,"d":"8.20"},"uH"]
[null,"IRIPPLE",{"v":2.613240418118467,"d":"2.61"},"A"]
[null,"VRIPPLE",{"v":54.4425087108014,"d":"54.44"},"mV"]
[]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":8.2,"d":"8.20"},"uH"]
[null,"Cout",{"v":20,"d":"20.00"},"uF"]
[null,"f0",{"v":12.427884031115202,"d":"12.43"},"kHz",null,"recommended range 10~15 kHz"]
[]
[null,"Timer (fixed)"]
[null,"Tprecharge",{"v":30,"d":"30.00"},"min"]
[null,"Tfastcharge",5,"hr"]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","0-60C"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (60C)",3.02,"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VCOOL",{"v":2.3331,"d":"2.33"},{"v":0.707,"d":"70.70%"}]
[null,"VWARM",{"v":1.5839999999999999,"d":"1.58"},{"v":0.48,"d":"48.00%"}]
[null,"R9",{"v":2.271567876373081,"d":"2.27"},"2.2 k-ohm"]
[null,"R10",{"v":6.85945733884236,"d":"6.86"},"6.8 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24600",32,"V"]

{"sheet":"bq24630","index":5,"n_rows":95,"n_cols":11,"rows_kept":95,"merged":[[17,1,17,3],[30,1,30,3],[37,1,37,3],[45,1,45,3],[52,1,52,3],[53,1,53,3],[61,1,61,3],[70,1,70,3],[73,5,73,7],[75,1,75,3],[78,1,78,3],[83,1,83,3],[93,1,93,3]],"flags":["formulas_cached_only"]}
[null,"LiFePO4 Charger bq24630 typical application circuit"]
{"$rows_empty":25}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Battery charge voltage setting"]
[null,"Cell count",3,"cell"]
[null,"Vcell",3.6,"V/cell"]
[null,"Vbat",10.8,"V"]
[null,"R1",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R2",500,"k-ohm"]
[]
[null,"Adaptor regulation current"]
[null,"Iadp",4,"A"]
[null,"RAC",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ACSET",{"v":0.8,"d":"0.800"},"V"]
[null,"R3",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R4",{"v":32.00000000000001,"d":"32.00"},"k-ohm"]
[]
[null,"Battery pre-charge/termination current setting"]
[null,"Iprechg (Iterm)",0.3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET2",0.3,"V",null,"Fixed Iprechg=125mA for 10mΩ sensing resistor"]
[null,"R5",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R6",{"v":10,"d":"10.00"},"k-ohm"]
[]
[null,"Battery fast-charge current setting"]
[null,"Ichg",3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V"]
[null,"V_ISET1",0.6,"V"]
[null,"R7",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R8",{"v":22.22222222222222,"d":"22.22"},"k-ohm"]
[]
[null,"Iripple_Lout",{"$nulls":3},"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Vin",28,"V",null,"Charge Current","2A","4A","6A","8A","10A"]
[null,"Vout (Vbat)",10.8,"V",null,"Output Inductor Lo","8.2mH","8.2mH","5.6mH","4.7mH","4.7mH"]
[null,"Duty",{"v":0.38571428571428573,"d":"0.386"},null,null,"Output Capacitor Co","20mF","20mF","30mF","40mF","40mF"]
[null,"Fs",300,"kHz",null,"Sense Resistor","10mW","10mW","10mW","10mW","10mW"]
[null,"Lout",{"v":8.2,"d":"8.20"},"uH"]
[null,"IRIPPLE",{"v":2.6968641114982583,"d":"2.70"},"A"]
[null,"VRIPPLE",{"v":56.184668989547035,"d":"56.18"},"mV"]
[]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":8.2,"d":"8.20"},"uH"]
[null,"Cout",{"v":20,"d":"20.00"},"uF"]
[null,"f0",{"v":12.427884031115202,"d":"12.43"},"kHz",null,"recommended range 10~15 kHz"]
[]
[null,"Precharge timer (fixed)"]
[null,"Tprecharge",{"v":30,"d":"30.00"},"min"]
[]
[null,"Fastcharge timer"]
[null,"Kttc",{"v":1.4,"d":"1.40"},"min/nF"]
[null,"Cttc",110,"nF"]
[null,"Tcharge",{"v":2.566666666666667,"d":"2.57"},"hr"]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","0-60C"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (60C)",3.02,"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VCOOL",{"v":2.3331,"d":"2.33"},{"v":0.707,"d":"70.70%"}]
[null,"VWARM",{"v":1.5839999999999999,"d":"1.58"},{"v":0.48,"d":"48.00%"}]
[null,"R9",{"v":2.271567876373081,"d":"2.27"},"2.2 k-ohm"]
[null,"R10",{"v":6.85945733884236,"d":"6.86"},"6.8 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24600",32,"V"]

{"sheet":"bq24640","index":6,"n_rows":70,"n_cols":11,"rows_kept":70,"merged":[[16,1,16,3],[25,1,25,3],[31,1,31,3],[32,1,32,3],[40,1,40,3],[49,1,49,3],[52,5,52,7],[58,1,58,3],[68,1,68,3]],"flags":["formulas_cached_only"]}
[null,"Supper cap charger bq24640 typical application circuit"]
{"$rows_empty":20}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Capacitor charge voltage setting"]
[null,"Cap count in series",3,"cap in series"]
[null,"Vcap for each cap",2.7,"V/cap"]
[null,"Vcap",8.100000000000001,"V"]
[null,"R1",{"v":105,"d":"105.0"},"k-ohm"]
[null,"R2",300.00000000000006,"k-ohm"]
[]
[null,"Capacitor charge current setting"]
[null,"Ichg",3,"A"]
[null,"RSR",10,"m-ohm"]
[null,"VREF",3.3,"V",null,"NO precharge, NO termination"]
[null,"V_ISET",0.6,"V"]
[null,"R7",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R8",{"v":22.22222222222222,"d":"22.22"},"k-ohm"]
[]
[null,"Iripple_Lout",{"$nulls":3},"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Vin",19,"V",null,"Charge Current","2A","4A","6A","8A","10A"]
[null,"Vout  (Vbat)",8.100000000000001,"V",null,"Output Inductor Lo","6.8mH","6.8mH","4.7mH","3.3mH","3.3mH"]
[null,"Duty",{"v":0.42631578947368426,"d":"0.426"},null,null,"Output Capacitor Co","20mF","20mF","30mF","40mF","40mF"]
[null,"Fs",600,"kHz",null,"Sense Resistor","10mW","10mW","10mW","10mW","10mW"]
[null,"Lout",{"v":6.8,"d":"6.80"},"uH"]
[null,"IRIPPLE",{"v":1.1389318885448916,"d":"1.14"},"A"]
[null,"VRIPPLE",{"v":11.863873839009289,"d":"11.86"},"mV"]
[]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":6.8,"d":"6.80"},"uH"]
[null,"Cout",{"v":20,"d":"20.00"},"uF"]
[null,"f0",{"v":13.647391865809526,"d":"13.65"},"kHz",null,"recommended range 12~17 kHz"]
[]
[]
[]
[]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","0-45C"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (45C)",{"v":4.911,"d":"4.91"},"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VLTF",{"v":2.4255,"d":"2.43"},{"v":0.735,"d":"73.50%"}]
[null,"VTCO",{"v":1.1351999999999998,"d":"1.14"},{"v":0.344,"d":"34.40%"}]
[null,"R9",{"v":9.261870542032382,"d":"9.26"},"9.31 k-ohm"]
[null,"R10",{"v":440.35294825762367,"d":"440.35"},"430 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24600",32,"V"]

{"sheet":"bq24650","index":7,"n_rows":72,"n_cols":10,"rows_kept":72,"merged":[[16,1,16,3],[26,1,26,3],[32,1,32,3],[33,1,33,3],[37,1,37,3],[42,1,42,3],[51,1,51,3],[56,1,56,3],[58,5,58,7],[60,1,60,3],[70,1,70,3]],"flags":["formulas_cached_only"]}
[null,"Solar charger bq24650 typical application circuit"]
{"$rows_empty":21}
[null,"User Input"]
[null,"Fixed Value"]
[null,"Calculated Value"]
[]
[null,"Battery charge voltage setting"]
[null,"Cell count",3,"cell"]
[null,"Vcell",4.2,"V/cell"]
[null,"Vbat",12.600000000000001,"V"]
[null,"R1",{"v":100,"d":"100.0"},"k-ohm"]
[null,"R2",500,"k-ohm"]
[]
[null,"Battery fast-charge current setting"]
[null,"Ichg",2,"A",null,"Iprechg=Iterm=Ichg/10"]
[null,"RSR",20,"m-ohm"]
[]
[null,"MPP voltage setting"]
[null,"VMPP",18,"V"]
[null,"R4",{"v":36,"d":"36.0"},"k-ohm"]
[null,"R3",504,"k-ohm"]
[]
[null,"Iripple_Lout"]
[null,"Vin",21,"V"]
[null,"Vout  (Vbat)",12.600000000000001,"V"]
[null,"Duty",{"v":0.6000000000000001,"d":"0.600"}]
[null,"Fs",600,"kHz",null,"Typical Inductor, Capacitor, and Sense Resistor Values as a function of charge current"]
[null,"Lout",{"v":15,"d":"15.00"},"uH",null,"Charge Current","1A","2A","4A","8A"]
[null,"IRIPPLE",0.56,"A",null,"Output Inductor Lo","15mH","10mH","6.8mH","3.3mH"]
[null,"VRIPPLE",{"v":11.666666666666664,"d":"11.67"},"mV",null,"Output Capacitor Co","10mF","15mF","20mF","40mF"]
[{"$nulls":5},"Sense Resistor","40mW","20mW","10mW","5mW"]
[null,"LC output filter resonant frequency"]
[null,"Lout",{"v":10,"d":"10.00"},"uH"]
[null,"Cout",{"v":15,"d":"15.00"},"uF"]
[null,"f0",{"v":12.994916299460883,"d":"12.99"},"kHz"]
[]
[null,"Timer (fixed)"]
[null,"Tprecharge",{"v":30,"d":"30.00"},"min"]
[null,"Tfastcharge",5,"hr",null,"recommended range 12~17 kHz"]
[]
[null,"TS resistor network"]
[null,"RTH (semitech)","103AT-2,3","0-45C"]
[null,"R_COLD (0C)",27.28,"k-ohm"]
[null,"R_HOT (45C)",{"v":4.911,"d":"4.91"},"k-ohm"]
[null,"VREF",{"v":3.3,"d":"3.30"},"V"]
[null,"VLTF",{"v":2.4255,"d":"2.43"},{"v":0.735,"d":"73.50%"}]
[null,"VTCO",{"v":1.4849999999999999,"d":"1.49"},{"v":0.45,"d":"45.00%"}]
[null,"R9",{"v":5.160749007904829,"d":"5.16"},"9.31 k-ohm"]
[null,"R10",{"v":30.11515021375447,"d":"30.12"},"430 k-ohm"]
[]
[null,"ACOV"]
[null,"bq24600",32,"V"]

{"sheet":"103AT","index":8,"n_rows":172,"n_cols":6,"rows_kept":172,"merged":[[10,4,10,5]],"flags":["formulas_cached_only"]}
["2000-03-01",null,"[ DATA FOR REFERENCE ]"]
[]
[null,"103AT-2,3"]
[null,"TEMPERATURE VS RESISTANCE CHARACTERISTICS [ITS-90]"]
[null,"Resistance: 10k Ohms at 25 deg. C"]
[null,"Resistance Tolerance:  + / - 1 %"]
[null,"B Value:  3435K at 25/85 deg. C"]
[null,"B Value Tolerance:    + / - 1 %"]
[]
[]
["Temp. (deg. C)","Rmax. (k Ohms)","Rst. (k Ohms)","Rmin. (k Ohms)","Tolerance (deg. C)"]
[-50,344.6,329.5,314.9,-0.8,{"v":0.8,"d":"+0.8"}]
[-49,325,310.9,297.3,-0.8,{"v":0.8,"d":"+0.8"}]
[-48,306.6,293.5,280.9,-0.8,{"v":0.8,"d":"+0.8"}]
[-47,289.4,277.2,265.4,-0.8,{"v":0.8,"d":"+0.8"}]
[-46,273.4,262,251,-0.8,{"v":0.8,"d":"+0.8"}]
[-45,258.3,247.7,237.4,-0.8,{"v":0.8,"d":"+0.8"}]
[-44,244.2,234.3,224.7,-0.8,{"v":0.8,"d":"+0.8"}]
[-43,231,221.7,212.8,-0.8,{"v":0.8,"d":"+0.8"}]
[-42,218.6,209.9,201.6,-0.8,{"v":0.8,"d":"+0.8"}]
[-41,207,198.9,191,-0.8,{"v":0.8,"d":"+0.8"}]
[-40,196,188.5,181.1,-0.8,{"v":0.8,"d":"+0.8"}]
[-39,185.5,178.5,171.6,-0.8,{"v":0.8,"d":"+0.8"}]
[-38,175.6,169,162.6,-0.8,{"v":0.8,"d":"+0.8"}]
[-37,166.3,160.2,154.2,-0.8,{"v":0.8,"d":"+0.8"}]
[-36,157.6,151.9,146.3,-0.7,{"v":0.8,"d":"+0.8"}]
[-35,149.4,144.1,138.8,-0.7,{"v":0.7,"d":"+0.7"}]
[-34,141.7,136.7,131.8,-0.7,{"v":0.7,"d":"+0.7"}]
[-33,134.5,129.8,125.2,-0.7,{"v":0.7,"d":"+0.7"}]
[-32,127.7,123.3,119,-0.7,{"v":0.7,"d":"+0.7"}]
[-31,121.2,117.1,113.1,-0.7,{"v":0.7,"d":"+0.7"}]
[-30,115.2,111.3,107.5,-0.7,{"v":0.7,"d":"+0.7"}]
[-29,109.4,105.7,102.2,-0.7,{"v":0.7,"d":"+0.7"}]
[-28,103.9,100.5,97.2,-0.7,{"v":0.7,"d":"+0.7"}]
[-27,98.68,95.52,92.45,-0.7,{"v":0.7,"d":"+0.7"}]
[-26,93.8,90.84,87.97,-0.7,{"v":0.7,"d":"+0.7"}]
[-25,89.2,86.43,83.73,-0.7,{"v":0.7,"d":"+0.7"}]
[-24,84.85,82.26,79.74,-0.7,{"v":0.7,"d":"+0.7"}]
[-23,80.76,78.33,75.96,-0.7,{"v":0.7,"d":"+0.7"}]
[-22,76.89,74.61,72.39,-0.7,{"v":0.7,"d":"+0.7"}]
[-21,73.23,71.1,69.01,-0.7,{"v":0.7,"d":"+0.7"}]
[-20,69.77,67.77,65.82,-0.6,{"v":0.7,"d":"+0.7"}]
[-19,66.44,64.57,62.74,-0.6,{"v":0.6,"d":"+0.6"}]
[-18,63.3,61.54,59.83,-0.6,{"v":0.6,"d":"+0.6"}]
[-17,60.32,58.68,57.07,-0.6,{"v":0.6,"d":"+0.6"}]
[-16,57.51,55.97,54.46,-0.6,{"v":0.6,"d":"+0.6"}]
[-15,54.85,53.41,51.99,-0.6,{"v":0.6,"d":"+0.6"}]
[-14,52.33,50.98,49.65,-0.6,{"v":0.6,"d":"+0.6"}]
[-13,49.95,48.68,47.43,-0.6,{"v":0.6,"d":"+0.6"}]
[-12,47.69,46.5,45.32,-0.6,{"v":0.6,"d":"+0.6"}]
[-11,45.55,44.43,43.33,-0.6,{"v":0.6,"d":"+0.6"}]
[-10,43.52,42.47,41.43,-0.6,{"v":0.6,"d":"+0.6"}]
[-9,41.55,40.57,39.6,-0.6,{"v":0.6,"d":"+0.6"}]
[-8,39.69,38.77,37.86,-0.6,{"v":0.6,"d":"+0.6"}]
[-7,37.92,37.06,36.21,-0.6,{"v":0.6,"d":"+0.6"}]
[-6,36.25,35.44,34.64,-0.6,{"v":0.6,"d":"+0.6"}]
[-5,34.66,33.9,33.15,-0.6,{"v":0.6,"d":"+0.6"}]
[-4,33.15,32.44,31.73,-0.5,{"v":0.5,"d":"+0.5"}]
[-3,31.72,31.05,30.39,-0.5,{"v":0.5,"d":"+0.5"}]
[-2,30.36,29.73,29.11,-0.5,{"v":0.5,"d":"+0.5"}]
[-1,29.06,28.48,27.89,-0.5,{"v":0.5,"d":"+0.5"}]
[0,27.83,27.28,26.74,-0.5,{"v":0.5,"d":"+0.5"}]
[1,26.65,26.13,25.62,-0.5,{"v":0.5,"d":"+0.5"}]
[2,25.52,25.03,24.55,-0.5,{"v":0.5,"d":"+0.5"}]
[3,24.44,23.99,23.54,-0.5,{"v":0.5,"d":"+0.5"}]
[4,23.42,23,22.57,-0.5,{"v":0.5,"d":"+0.5"}]
[5,22.45,22.05,21.66,-0.5,{"v":0.5,"d":"+0.5"}]
[6,21.53,21.15,20.78,-0.5,{"v":0.5,"d":"+0.5"}]
[7,20.64,20.3,19.95,-0.5,{"v":0.5,"d":"+0.5"}]
[8,19.81,19.48,19.15,-0.5,{"v":0.5,"d":"+0.5"}]
[9,19.01,18.7,18.39,-0.4,{"v":0.5,"d":"+0.5"}]
[10,18.25,17.96,17.67,-0.4,{"v":0.4,"d":"+0.4"}]
[11,17.51,17.24,16.97,-0.4,{"v":0.4,"d":"+0.4"}]
[12,16.81,16.56,16.3,-0.4,{"v":0.4,"d":"+0.4"}]
[13,16.14,15.9,15.67,-0.4,{"v":0.4,"d":"+0.4"}]
[14,15.5,15.28,15.06,-0.4,{"v":0.4,"d":"+0.4"}]
[15,14.89,14.69,14.48,-0.4,{"v":0.4,"d":"+0.4"}]
[16,14.31,14.12,13.92,-0.4,{"v":0.4,"d":"+0.4"}]
[17,13.75,13.58,13.39,-0.4,{"v":0.4,"d":"+0.4"}]
[18,13.22,13.06,12.89,-0.4,{"v":0.4,"d":"+0.4"}]
[19,12.72,12.56,12.4,-0.4,{"v":0.4,"d":"+0.4"}]
[20,12.24,12.09,11.94,-0.4,{"v":0.4,"d":"+0.4"}]
[21,11.77,11.63,11.5,-0.3,{"v":0.4,"d":"+0.4"}]
[22,11.32,11.2,11.07,-0.3,{"v":0.3,"d":"+0.3"}]
[23,10.9,10.78,10.66,-0.3,{"v":0.3,"d":"+0.3"}]
[24,10.49,10.38,10.27,-0.3,{"v":0.3,"d":"+0.3"}]
[25,10.1,10,9.9,-0.3,{"v":0.3,"d":"+0.3"}]
[26,9.732,9.632,9.532,-0.3,{"v":0.3,"d":"+0.3"}]
[27,9.38,9.281,9.18,-0.3,{"v":0.3,"d":"+0.3"}]
[28,9.043,8.944,8.844,-0.4,{"v":0.4,"d":"+0.4"}]
[29,8.721,8.622,8.522,-0.4,{"v":0.4,"d":"+0.4"}]
[30,8.411,8.313,8.214,-0.4,{"v":0.4,"d":"+0.4"}]
[31,8.112,8.014,7.916,-0.4,{"v":0.4,"d":"+0.4"}]
[32,7.826,7.728,7.631,-0.4,{"v":0.4,"d":"+0.4"}]
[33,7.551,7.454,7.358,-0.4,{"v":0.4,"d":"+0.4"}]
[34,7.288,7.192,7.096,-0.4,{"v":0.4,"d":"+0.4"}]
[35,7.035,6.94,6.845,-0.4,{"v":0.4,"d":"+0.4"}]
[36,6.793,6.699,6.605,-0.4,{"v":0.4,"d":"+0.4"}]
[37,6.56,6.467,6.374,-0.5,{"v":0.5,"d":"+0.5"}]
[38,6.337,6.245,6.153,-0.5,{"v":0.5,"d":"+0.5"}]
[39,6.123,6.032,5.941,-0.5,{"v":0.5,"d":"+0.5"}]
[40,5.918,5.827,5.738,-0.5,{"v":0.5,"d":"+0.5"}]
[41,5.718,5.629,5.54,-0.5,{"v":0.5,"d":"+0.5"}]
[42,5.526,5.438,5.351,-0.5,{"v":0.5,"d":"+0.5"}]
[43,5.342,5.255,5.169,-0.5,{"v":0.5,"d":"+0.5"}]
[44,5.165,5.08,4.994,-0.5,{"v":0.5,"d":"+0.5"}]
[45,4.995,4.911,4.827,-0.6,{"v":0.6,"d":"+0.6"}]
[46,4.832,4.749,4.666,-0.6,{"v":0.6,"d":"+0.6"}]
[47,4.675,4.593,4.511,-0.6,{"v":0.6,"d":"+0.6"}]
[48,4.524,4.443,4.363,-0.6,{"v":0.6,"d":"+0.6"}]
[49,4.379,4.299,4.22,-0.6,{"v":0.6,"d":"+0.6"}]
[50,4.239,4.16,4.082,-0.6,{"v":0.6,"d":"+0.6"}]
[51,4.103,4.026,3.949,-0.6,{"v":0.6,"d":"+0.6"}]
[52,3.972,3.896,3.82,-0.6,{"v":0.6,"d":"+0.6"}]
[53,3.846,3.771,3.697,-0.7,{"v":0.7,"d":"+0.7"}]
[54,3.725,3.651,3.578,-0.7,{"v":0.7,"d":"+0.7"}]
[55,3.609,3.536,3.464,-0.7,{"v":0.7,"d":"+0.7"}]
[56,3.496,3.425,3.354,-0.7,{"v":0.7,"d":"+0.7"}]
[57,3.388,3.318,3.248,-0.7,{"v":0.7,"d":"+0.7"}]
[58,3.284,3.215,3.146,-0.7,{"v":0.7,"d":"+0.7"}]
[59,3.184,3.116,3.048,-0.7,{"v":0.7,"d":"+0.7"}]
[60,3.087,3.02,2.954,-0.7,{"v":0.8,"d":"+0.8"}]
[61,2.993,2.927,2.862,-0.8,{"v":0.8,"d":"+0.8"}]
[62,2.902,2.838,2.774,-0.8,{"v":0.8,"d":"+0.8"}]
[63,2.815,2.751,2.688,-0.8,{"v":0.8,"d":"+0.8"}]
[64,2.731,2.668,2.606,-0.8,{"v":0.8,"d":"+0.8"}]
[65,2.65,2.588,2.527,-0.8,{"v":0.8,"d":"+0.8"}]
[66,2.571,2.511,2.451,-0.8,{"v":0.8,"d":"+0.8"}]
[67,2.496,2.436,2.378,-0.8,{"v":0.9,"d":"+0.9"}]
[68,2.423,2.364,2.307,-0.9,{"v":0.9,"d":"+0.9"}]
[69,2.352,2.295,2.238,-0.9,{"v":0.9,"d":"+0.9"}]
[70,2.284,2.228,2.172,-0.9,{"v":0.9,"d":"+0.9"}]
[71,2.218,2.163,2.108,-0.9,{"v":0.9,"d":"+0.9"}]
[72,2.154,2.1,2.046,-0.9,{"v":0.9,"d":"+0.9"}]
[73,2.092,2.039,1.986,-0.9,{"v":0.9,"d":"+0.9"}]
[74,2.033,1.98,1.929,-0.9,{"v":1,"d":"+1.0"}]
[75,1.975,1.924,1.873,{"v":-1,"d":"-1.0"},{"v":1,"d":"+1.0"}]
[76,1.92,1.869,1.819,{"v":-1,"d":"-1.0"},{"v":1,"d":"+1.0"}]
[77,1.866,1.816,1.767,{"v":-1,"d":"-1.0"},{"v":1,"d":"+1.0"}]
[78,1.814,1.765,1.717,{"v":-1,"d":"-1.0"},{"v":1,"d":"+1.0"}]
[79,1.764,1.716,1.668,{"v":-1,"d":"-1.0"},{"v":1,"d":"+1.0"}]
[80,1.715,1.668,1.621,{"v":-1,"d":"-1.0"},{"v":1,"d":"+1.0"}]
[81,1.668,1.622,1.576,{"v":-1,"d":"-1.0"},{"v":1.1,"d":"+1.1"}]
[82,1.622,1.577,1.532,-1.1,{"v":1.1,"d":"+1.1"}]
[83,1.578,1.533,1.489,-1.1,{"v":1.1,"d":"+1.1"}]
[84,1.535,1.492,1.448,-1.1,{"v":1.1,"d":"+1.1"}]
[85,1.494,1.451,1.409,-1.1,{"v":1.1,"d":"+1.1"}]
[86,1.454,1.412,1.37,-1.1,{"v":1.1,"d":"+1.1"}]
[87,1.415,1.373,1.332,-1.1,{"v":1.1,"d":"+1.1"}]
[88,1.377,1.336,1.296,-1.2,{"v":1.2,"d":"+1.2"}]
[89,1.341,1.301,1.261,-1.2,{"v":1.2,"d":"+1.2"}]
[90,1.305,1.266,1.227,-1.2,{"v":1.2,"d":"+1.2"}]
[91,1.271,1.232,1.194,-1.2,{"v":1.2,"d":"+1.2"}]
[92,1.238,1.2,1.162,-1.2,{"v":1.2,"d":"+1.2"}]
[93,1.205,1.168,1.131,-1.2,{"v":1.2,"d":"+1.2"}]
[94,1.174,1.137,1.101,-1.2,{"v":1.3,"d":"+1.3"}]
[95,1.144,1.108,1.072,-1.3,{"v":1.3,"d":"+1.3"}]
[96,1.115,1.079,1.044,-1.3,{"v":1.3,"d":"+1.3"}]
[97,1.086,1.051,1.017,-1.3,{"v":1.3,"d":"+1.3"}]
[98,1.059,1.024,0.9913,-1.3,{"v":1.3,"d":"+1.3"}]
[99,1.032,0.9984,0.9658,-1.3,{"v":1.3,"d":"+1.3"}]
[100,1.006,0.9731,0.9411,-1.3,{"v":1.4,"d":"+1.4"}]
[101,0.9808,0.9484,0.917,-1.4,{"v":1.4,"d":"+1.4"}]
[102,0.9563,0.9246,0.8937,-1.4,{"v":1.4,"d":"+1.4"}]
[103,0.9326,0.9014,0.8711,-1.4,{"v":1.4,"d":"+1.4"}]
[104,0.9096,0.8789,0.8492,-1.4,{"v":1.4,"d":"+1.4"}]
[105,0.8873,0.8572,0.8279,-1.4,{"v":1.4,"d":"+1.4"}]
[106,0.8656,0.836,0.8073,-1.4,{"v":1.5,"d":"+1.5"}]
[107,0.8446,0.8155,0.7873,-1.5,{"v":1.5,"d":"+1.5"}]
[108,0.8242,0.7956,0.7679,-1.5,{"v":1.5,"d":"+1.5"}]
[109,0.8044,0.7763,0.7491,-1.5,{"v":1.5,"d":"+1.5"}]
[110,0.7851,0.7576,0.7308,-1.5,{"v":1.5,"d":"+1.5"}]