
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "HC-SR04" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0.0 5.0813 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "HC-SR04" (id 1) (at 0.0 -10.163 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "HC-SR04:XCVR_HC-SR04" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "SparkFun Electronics" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            HC-SR04 Ultrasonic Sensor Qwiic Platform Evaluation Expansion Board\n                        \n" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "None" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/HC-SR04/SparkFun/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/HC-SR04/SparkFun/view-part/?ref=snap" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "HC-SR04" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "Not in stock" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Osepp" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "HC-SR04_0_0"
      (rectangle (start -8.881784197e-16 -7.62) (end 10.16 5.08)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at -5.08 2.54 0) (length 5.08)
        (name "VCC"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -5.08 0.0 0) (length 5.08)
        (name "TRIG"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "ECHO"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)