
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "RASPBERRY_PI_ZERO_2_W" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -25.42 39.3962 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "RASPBERRY_PI_ZERO_2_W" (id 1) (at -25.4191 -40.6687 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "RASPBERRY_PI_ZERO_2_W:MODULE_RASPBERRY_PI_ZERO_2_W" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Raspberry Pi" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            At the heart of Raspberry Pi Zero 2 W is RP3A0, a custom-built system-in-package designed by Raspberry Pi in the UK.\n                        \n" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "None" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/RASPBERRY%20PI%20ZERO%202%20W/Raspberry+Pi/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "April 2024" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RASPBERRY%20PI%20ZERO%202%20W/Raspberry+Pi/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "RASPBERRY PI ZERO 2 W" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Raspberry Pi" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "RASPBERRY_PI_ZERO_2_W_0_0"
      (rectangle (start -25.4 -38.1) (end 25.4 38.1)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 30.48 35.56 180.0) (length 5.08)
        (name "5V_2"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 30.48 180.0) (length 5.08)
        (name "3V3_1"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 22.86 0) (length 5.08)
        (name "GPIO2/SDA1"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 33.02 180.0) (length 5.08)
        (name "5V_4"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 20.32 0) (length 5.08)
        (name "GPIO3/SCL"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -17.78 180.0) (length 5.08)
        (name "GND_6"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 17.78 0) (length 5.08)
        (name "GPIO4/GPIO_GCLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 -7.62 0) (length 5.08)
        (name "GPIO14/TXD0"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -20.32 180.0) (length 5.08)
        (name "GND_9"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 22.86 180.0) (length 5.08)
        (name "GPIO15/RXD0"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 17.78 180.0) (length 5.08)
        (name "GPIO17/GPIO_GEN0"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 15.24 180.0) (length 5.08)
        (name "GPIO18/GPIO_GEN1"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 -7.62 180.0) (length 5.08)
        (name "GPIO27/GPIO_GEN2"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -22.86 180.0) (length 5.08)
        (name "GND_14"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 5.08 180.0) (length 5.08)
        (name "GPIO22/GPIO_GEN3"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 2.54 180.0) (length 5.08)
        (name "GPIO23/GPIO_GEN4"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 27.94 180.0) (length 5.08)
        (name "3V3_17"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 0.0 180.0) (length 5.08)
        (name "GPIO24/GPIO_GEN5"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 2.54 0) (length 5.08)
        (name "GPIO10/SPI_MOSI"
          (effects (font (size 1.016 1.016)))
        )
        (number "19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -25.4 180.0) (length 5.08)
        (name "GND_20"
          (effects (font (size 1.016 1.016)))
        )
        (number "20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 5.08 0) (length 5.08)
        (name "GPIO9/SPI_MISO"
          (effects (font (size 1.016 1.016)))
        )
        (number "21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 -2.54 180.0) (length 5.08)
        (name "GPIO25/GPIO_GEN6"
          (effects (font (size 1.016 1.016)))
        )
        (number "22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 0.0 0) (length 5.08)
        (name "GPIO11/SPI_SCLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "23"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 7.62 0) (length 5.08)
        (name "GPIO8/SPI_~{CE0}"
          (effects (font (size 1.016 1.016)))
        )
        (number "24"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -27.94 180.0) (length 5.08)
        (name "GND_25"
          (effects (font (size 1.016 1.016)))
        )
        (number "25"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 10.16 0) (length 5.08)
        (name "GPIO7/SPI_~{CE1}"
          (effects (font (size 1.016 1.016)))
        )
        (number "26"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 -12.7 0) (length 5.08)
        (name "ID_SD"
          (effects (font (size 1.016 1.016)))
        )
        (number "27"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 -15.24 0) (length 5.08)
        (name "ID_SC"
          (effects (font (size 1.016 1.016)))
        )
        (number "28"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 15.24 0) (length 5.08)
        (name "GPIO5"
          (effects (font (size 1.016 1.016)))
        )
        (number "29"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -30.48 180.0) (length 5.08)
        (name "GND_30"
          (effects (font (size 1.016 1.016)))
        )
        (number "30"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 12.7 0) (length 5.08)
        (name "GPIO6"
          (effects (font (size 1.016 1.016)))
        )
        (number "31"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 -2.54 0) (length 5.08)
        (name "GPIO12"
          (effects (font (size 1.016 1.016)))
        )
        (number "32"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -30.48 -5.08 0) (length 5.08)
        (name "GPIO13"
          (effects (font (size 1.016 1.016)))
        )
        (number "33"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -33.02 180.0) (length 5.08)
        (name "GND_34"
          (effects (font (size 1.016 1.016)))
        )
        (number "34"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 12.7 180.0) (length 5.08)
        (name "GPIO19"
          (effects (font (size 1.016 1.016)))
        )
        (number "35"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 20.32 180.0) (length 5.08)
        (name "GPIO16"
          (effects (font (size 1.016 1.016)))
        )
        (number "36"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 -5.08 180.0) (length 5.08)
        (name "GPIO26"
          (effects (font (size 1.016 1.016)))
        )
        (number "37"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 10.16 180.0) (length 5.08)
        (name "GPIO20"
          (effects (font (size 1.016 1.016)))
        )
        (number "38"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 30.48 -35.56 180.0) (length 5.08)
        (name "GND_39"
          (effects (font (size 1.016 1.016)))
        )
        (number "39"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 30.48 7.62 180.0) (length 5.08)
        (name "GPIO21"
          (effects (font (size 1.016 1.016)))
        )
        (number "40"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)